MaK G400B Diesel switcher locomotive
CFL livery
Build for DSB railways by Siemens/Vossloh
in service in CFL Luxemburg Railways
and in european private company
Construction dates: 1996-1999
Engine: MTU 8V 183 TD13 330kW
Mechanical transmission with hydraulic coupler.
Max speed: 60 km/h
----------------
Installation
1-Unzip (with option - "keep folder" active)the file in the folder Trainsimulator\trains\trainset\
The folder MAKG400 will be created.
2-Create a consist with this locomotive named "CFL G400"
----------------
Model build with TSM from Abacus
March 7, 2003
version 1.0
Author & copyright: Pierre Gauriat
email : pierreg@free.fr
website : http://ajtrainsim.free.fr/
This model may not be sold or distributed in any way without the authors permission.
